[DCNND2]
 Type = NDIS
 Title = "DigitalChina DCN-530TX Fast Ethernet Adapter."
 Version = 1.00
 DriverName = DCNND2$
 XPORTS = NETBEUI LANDD

[File]
 Name = DCNND2.OS2
 Path = IBMCOM\MACS

[Slot]
 display = "Network Adapter Slot ID."
 type = Decimal
 default = "1"
 range = 1 - 4
 step = 1
 optional = Yes
 editable = Yes
 virtual = No
 help = "This parameter specifies which network adapter is used by the driver.
 If you have only one DigitalChina DCN-530TX Fast Ethernet Adapter in your
 machine, this parameter is unnecessary!! For two or more DigitalChina DCN-530TX
 Fast Ethernet Adapter, this parameters is required and cannot be omitted from
 PROTOCOL.INI. The slot ID. for the first LAN card is 1, for the second is 2,
 and 3 for the third, etc.  Default value is 1."

[MEDIA]
 display = "Physical Medium Type"
 type = String
 strlength = 14
 default = "AUTODETECT"
 set = AUTODETECT, UTP, UTP_FD, UTP_100,UTP_100FD
 optional = No
 editable = Yes
 virtual = No
 help = "This parameter specifies the physical media that the LAN card is
 attached.  The keyword AUTODETECT means driver will auto sense the physical
 media during card initialization. UTP means twisted-pair (RJ-45 or 10BaseT),
 and UTP_100 means Fast Ethernet. If you want to enable full duplex function
 of the LAN  card, you have to choose UTP_FD or UTP_100FD as the medium type.
 The default value is AUTODETECT."

