
          DigitalChina DCN-530TX Fast Ethernet Adapter
                 Windows 95 Driver Installation

  Contents:
  ---------
   (A) Installing the driver in Microsoft Windows 95
   (B) Configuring the driver in Microsoft Windows 95
   
(A) Installing the driver in Microsoft Windows 95
================================================================
    1. Make sure your computer is power-off.
    2. Plug the adapter into one of the PCI slots of your PC.
    3. Turn the power ON, then boot into Windows 95.
    4. Windows 95 will find the new hardware automatically,
       then "New Hardware Found" dialog box will appear.
    5. Select "Driver from disk provided by the hardware
       manufacturer" and click "OK".
    6. Insert the Driver Diskette.
    7. Type Path "X:\WIN95" in the text box, then click "OK".

      Notice: X: means the floppy drive containing the drivers,
      such as: A:, or B: etc.

    8. Windows 95 will prompt with "DigitalChina DCN-530TX Fast
       Ethernet Adapter" in the dialog box.
    9. Click "OK" button, then Windows 95 will copy the driver.
   10. After finishing file copying, Windows 95 will ask
       you to restart the system. Remove the Driver Diskette
       and click "Yes" to reboot.

(B) Configuring the driver on Microsoft Windows 95
================================================================

    1. Double click the "My Computer" icon.
    2. Double click the "Control Panel" icon.
    3. Double click the "Network" icon.
    4. Select the "DigitalChina DCN-530TX Fast Ethernet Adapter"
       item, then click the "Properties" button.
    5. Click the "Advanced" tab.
    6. There are 1 items in the "Property" box.

       ------Media Type      
       .Specify the media type for the adapter.
       .Default: AutoSense
       
    7. Click "OK" button to return to "Network" dialog box.
    8. Click "OK" button and restart your PC to make the new
       configuration take effect.

Trademarks:
Microsoft Windows 95 is a trademark of Microsoft Corporation.
