
  神州数码DCN-530TX快速以太网卡NDIS/2 DOS驱动在LAN Manager下的安装

  内容：
  -----------
  (A)NDIS 2驱动在LAN Manager v2.0下安装
  (B)NDIS 2驱动在LAN Manager v2.1下安装
  (C)NDIS 2驱动在LAN Manager v2.2下安装

  (A)NDIS 2驱动在LAN Manager v2.0下安装
  ===========================================
  1.在LAN Manager目录下键入“Setup”并回车。

  2.在“Action”项中选择“Import Network Drivers...”。按回车键继续。

  3.插入网卡驱动程序磁盘，按回车键，在界面上将显示网卡驱动列表。

  4.按空格键来选择对应网卡“DigitalChina DCN-530TX Fast Ethernet Adapter”，按回车键来确认您的选择。

  5.根据屏幕提示完成操作，直到网络驱动显示在屏幕上。

  6.如果系统要识别网卡，请选择“DigitalChina DCN-530TX Fast Ethernet Adapter”来确认。

  7.选择<Add Driver>和<Add Protocol>选项。然后选择<OK>来确认您的选择。工作站的基本参数将显示在界面上。

  8.按照界面上所有的提示来完成安装。选择<OK>来确认选择。

  9.从<Action Menu>中选择<Save>来保存所有选择。

  10.按F3退出。

  (B)NDIS 2驱动在LAN Manager v2.1下安装
  ===========================================
  1.在LAN Manager目录下键入“lmsetup”，并按回车键。界面上将显示Microsoft LAN Manager安装界面。

  2.在“Configuration”项中选择“Network Drivers...”。按回车键来确认您的选择。

  3.选择<Add New Config>，按回车键将显示网卡驱动列表。

  4.选择<Other Driver>，按回车键。

  5.插入网卡驱动程序磁盘，指定驱动程序位置，选择<OK>继续。

  6.选择“DigitalChina DCN-530TX Fast Ethernet Adapter”，选择<OK>来确认您的选择。

  7.选择相关的协议。用空格键加亮您的选择。

  8.选择<OK>来确认您的选择。界面将显示配置完成信息。

  9.选择<Save>来保存配置信息。

  10.按F3退出。

  (C)NDIS 2驱动在LAN Manager v2.2下安装
  ============================================
  1.在LAN Manager目录(C:\LANMAN.DOS)中键入“Setup”，并按回车键，将显示Microsoft LAN Manager安装界面。

  2.从“Configuration”中选择“Network Drivers”。按回车键来确认选择。

  3.选择“Add New Config”，并按回车键来显示网卡驱动列表。

  4.插入网卡驱动程序磁盘，指定驱动程序位置。

  5.选择<Other Driver>，按回车键。

  6.选择“DigitalChina DCN-530TX Fast Ethernet Adapter”，选择<OK>来确认您的选择。

  7.选择相应的协议。用空格键加亮您的选择。如果您选择了TCP/IP协议，将被提示输入IP地址、子网掩码、缺省网关(路由接口)。
    缺省条件下，工作站的Netbios session数被设置为6。细情请参考Microsoft LAN Nanager安装手册或联机帮助。

  8.选择<OK>来确认您的选择。界面将显示配置完成信息。

  9.选择<Save>来保存配置信息。

  10.按F3退出。

  配置文件范例：
  ======================
  LAN Manager 2.0

  CONFIG.SYS File

      LASTDRIVE=Z
      BUFFERS = 35
      FILES = 35
      SHELL=C:\DOS50\COMMAND.COM C:\DOS50 /p /E:1024
      DEVICE=C:\HIMEM.SYS
      DEVICE=C:\DOS50\SETVER.EXE
      DOS=HIGH,UMB
      DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /i:C:\LANMAN.DOS
      DEVICE=C:\LANMAN.DOS\DRIVERS\DC\DCNND2\DCNND2.DOS
      DEVICE=C:\LANMAN.DOS\DRIVERS\PROTOCOL\NETBEUI\NETBEUI.DOS

  PROTOCOL.INI File

      [PROTOCOL MANAGER]
       DRIVERNAME = PROTMAN$
      [NETBEUI_XIF]
       Drivername = netbeui$
       BINDINGS = "DCNND2_NIF"
      [DCNND2_NIF]
     ;----------------------------------------------------------------------
     ; Sample Protocol.ini file for DCNND2 NDIS 2 driver
     ;----------------------------------------------------------------------
       DriverName = DCNND2$
     ; Slot = 1            ;; {1-4}
     ; MEDIA = AUTODETECT
     ;; {MEDIA = UTP, UTP_FD, UTP_100,UTP_100FD, AUTODETECT}
     ;----------------------------------------------------------------------
     ; End of this sample file

  AUTOEXEC.BAT File

        @echo off
        PROMPT $P$G
        PATH=c:\PE2;C:\DOS50;C:\NC;
        APPEND=C:\PE2;C:\DOS50;
        REM ====== LANMAN 2.0 === DO NOT MODIFY BETWEEN THESE LINES
        SET PATH=C:\LANMAN.DOS\NETPROG;%PATH%
        C:\LANMAN.DOS\DRIVERS\PROTMAN\NETBIND
        NET START WORKSTATION
        REM ====== LANMAN 2.0 === DO NOT MODIFY BETWEEN THESE LINES

  LAN Manager 2.1 or LAN Manager 2.2

  CONFIG.SYS File

        LASTDRIVE=Z
        BUFFERS = 35
        FILES = 35
        SHELL=C:\DOS62\COMMAND.COM C:\DOS62 /p /E:1024
        DEVICE=C:\HIMEM.SYS
        REM DEVICE=C:\LANMAN.DOS\DRIVERS\DOSUTILS\EMM386.EXE NoEMS ;;delete
                                                                   ;;this
                                                                   ;;line
        DEVICE=C:\DOS62\SETVER.EXE
        DOS=HIGH,UMB
        DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /i:C:\LANMAN.DOS
        DEVICE=C:\LANMAN.DOS\DRIVERS\DC\DCNND2\DCNND2.DOS

  PROTOCOL.INI File

        [PROTMAN]
         DRIVERNAME = PROTMAN$
         DYNAMIC = YES
         PRIORITY = NETBEUI
        [NETBEUI_XIF]
         Drivername = netbeui$
         SESSIONS = 6
         NCBS = 12
         BINDINGS = "DCNND2_NIF"
         LANABASE = 0

        [DCNND2_NIF]
        ;-------------------------------------------------------------------
        ; Sample Protocol.ini file for DCNND2 NDIS 2 driver
        ;-------------------------------------------------------------------
          DriverName = DCNND2$
        ; Slot = 1            ;; {1-4}
        ; MEDIA = AUTODETECT
        ;; {MEDIA = UTP, UTP_FD, UTP_100,UTP_100FD, AUTODETECT}
        ;-------------------------------------------------------------------
        ; End of this sample file

  AUTOEXEC.BAT File

        @echo off
        PROMPT $P$G
        PATH=c:\PE2;C:\DOS62;C:\NC;
        APPEND=C:\PE2;C:\DOS62;
        @REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES
        @REM=== LANMAN 2.1 ===
        SET PATH=C:\LANMAN.DOS\NETPROG;%PATH%
        NET START WORKSTATION
        LOAD NETBEUI
        @REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES
        @REM === LANMAN 2.1 ===
